        #
        | README file for
        |
        | ELSA MicroLink ISDN/MC
        | Version 2.50
        |
        | Copyright (c) 1993-99 ELSA AG, Aachen (Germany)
        |
        | ELSA AG                    Internet   : http://www.elsa.de
        | Sonnenweg 11               LocalWeb   : +49-(0)241-938800
        | D-52070 Aachen
        |
        | ELSA Inc.                  Internet   : http://www.elsa.com
        | 2231 Calle De Luna
        | Santa Clara, CA 95054
        | USA
        |
        | ELSA Asia Inc.             Internet   : http://www.elsa.com
        | 7F-11, No. 188, Sec. 5
        | Nanking East Road
        | Taipei 105
        | Taiwan, R. O. C.
        |
        | ELSA Japan Inc.            Internet   : http://www.elsa.com
        | Mita Suzuki Building 3F
        | 5-20-14 Shiba, Minato-ku
        | Tokyo 108-0014
        | Japan
        |
        | 07/30/1999



- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

        Table of Contents

        1.      Overview
        2.      Contents
        3.      Installation
        4.      Notes

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

1.      Overview:

        This file contains notes and changes to the MicroLink
        ISDN drivers.

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

2.      Contents:

        The driver disk contains the following files:

        README.TXT   this file
        LIESMICH.TXT german version of the readme.txt file

               - - - - - - - - - - - - - - - - - - - - - - - -

2.1     Driver for CAPI 2.0 and DSS1 (EURO-ISDN):

        CSSELMC.VXD  CAPI version 2.0 driver for ELSA MicroLink ISDN/MC
        D channel protocol : DSS1 (EURO-ISDN)
        B channel protocols: HDLC transparent, bit transparent,
                             X.75, T.70NL, V.120
                             ISO 8208 (X.25), T.90

               - - - - - - - - - - - - - - - - - - - - - - - -

2.2     Driver for CAPI 2.0 and 1TR6 (national ISDN):

        CSS1TMC.VXD  CAPI version 2.0 driver for ELSA MicroLink ISDN/MC
        D channel protocol : 1TR6 (national ISDN)
        B channel protocols: HDLC transparent, bit transparent,
                             X.75, T.70NL, V.120
                             ISO 8208 (X.25), T.90

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

3.      Installation:

        a.) Install the PCMCIA-Controller

            For installing the PCMCIA-Controller you must choose
            the hardware-assitent.

        b.) Install the driver for the MicroLink ISDN board

            Reboot your system and put the MicroLink ISDN board
            into the pcmcia-slot.
            The driver for your ISDN-Board will be installed
            automatically.

        c.) Restart your computer.

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

4.      Notes:

        The latest information you will always find in the
        ELSA LocalWeb or on our homepage.

               - - - - - - - - - - - - - - - - - - - - - - - -

        V.120 under CAPI 2.0 and CFOS (version newer than 07/15/96):

        Enter the following AT-command:

            AT B12 S17=1 S76=1

        Now, the ISDN adapter board tries to get a V.120 connection
        erverytime you dial "ATDn" (n = number)..

        If you want to get back to X.75 mode, you have to enter:

            AT&F

               - - - - - - - - - - - - - - - - - - - - - - - -

        Have fun with your ELSA ISDN board.
