; Windows Modem Setup File
; Copyright (c) 1993-2000 ELSA AG
; Manufacturer:   ELSA AG
; 200900, clubberi	INF-File ML ISDN Office
;
; Serial Modem installer for Windows
; Device Properties, Responses, etc.
;
;-----------------------------------------------------------------------------


[Version]
Signature="$CHICAGO$"
Class=Modem
ClassGUID={4D36E96D-E325-11CE-BFC1-08002BE10318}
Provider=%Mfg%
;Catalogfile=mdmelsi3.cat
DriverVer = 01/29/2001,1.3.0.2

[ControlFlags]
ExcludeFromSelect= SERENUM\ELS8844    		;Modem115

[Modem115.NoResDup]
UNIMODEMBBEB0862

[PortDriver]
HKR, , PortDriver, , wdmmdmld.vxd
HKR, , Contention, 0,

[Manufacturer]
%Mfg% = Models

[Models]
%Modem115PNP% = Modem115, SERENUM\ELS8844 ; ELSA MicroLink ISDN Office
%Modem115% = Modem115, UNIMODEMBBEB0862   ; PPP
%Modem114% = Modem114, UNIMODEMBBEB0862   ; X75
%Modem113% = Modem113, UNIMODEMBBEB0862   ; V120
%Modem112% = Modem112, UNIMODEMBBEB0862   ; Auto-Fallback
%Modem111% = Modem111, UNIMODEMBBEB0862   ; Btx
%Modem110% = Modem110, UNIMODEMBBEB0862   ; V110

; Installation sections

[Modem115]       ; ELSA MicroLink ISDN Office
DriverVer = 01/29/2001,1.3.0.2
AddReg=Main, Properties, Responses, PPP.AddReg, ISDN, External

[Modem114]       ; X75
DriverVer = 01/29/2001,1.3.0.2
AddReg=Main, Properties, Responses, X75.AddReg, ISDN, External

[Modem113]       ; V120
DriverVer = 01/29/2001,1.3.0.2
AddReg=Main, Properties, Responses, V120.AddReg, ISDN, External

[Modem112]       ; Fallback
DriverVer = 01/29/2001,1.3.0.2
AddReg=Main, Properties, Responses, Fallback.AddReg, ISDN, External

[Modem111]       ; Btx
DriverVer = 01/29/2001,1.3.0.2
AddReg=Main, Properties, Responses, BTX.AddReg, ISDN, External

[Modem110]       ; V110
DriverVer = 01/29/2001,1.3.0.2
AddReg=Main, Properties, Responses, V110.AddReg, ISDN, External

; User visible strings

[Strings]
Mfg = "ELSA"

; Model strings
Modem115PNP=	"ELSA MicroLink ISDN Office"
Modem115=	"ELSA MicroLink ISDN Office PPP"
Modem114=	"ELSA MicroLink ISDN Office X.75"
Modem113=	"ELSA MicroLink ISDN Office V.120"
Modem112=	"ELSA MicroLink ISDN Office X75FB2"
Modem111=	"ELSA MicroLink ISDN Office Btx"
Modem110=	"ELSA MicroLink ISDN Office V.110"



; AddReg sections


[Main]
HKR,,FriendlyDriver,,unimodem.vxd
HKR,,DevLoader,,*vcomm
HKR,,PortSubClass,1,02
HKR,,ConfigDialog,,modemui.dll
HKR,,EnumPropPages,,"modemui.dll,EnumPropPages"
HKR, Init,      1,, "AT&FE0&D2&C1V1Q0\V8S0=0<cr>"
HKR, Monitor,   1,, "ATS0=0<cr>"
HKR, Monitor,   2,, "None"
HKR, Hangup,    1,, "ATH<cr>"
HKR, Answer,    1,, "ATA<cr>"
HKR,, Reset,, "ATZ<cr>"
HKR, Settings, Prefix,, "AT"
HKR, Settings, Terminator,, "<cr>"
HKR, Settings, DialPrefix,, "D"
HKR, Settings, DialSuffix,, ""
HKR, Settings, FlowControl_Off,, "+ifc=0,0;"
HKR, Settings, FlowControl_Hard,, "+ifc=2,2;"
;HKR, Settings, FlowControl_Soft,, "+ifc=1,1;"
HKR,, InactivityScale,1,0a,00,00,00
HKR, Settings, InactivityTimeout,, "S30=<#>"


[Properties]
HKR,, Properties, 1, 00,00,00,00, 00,00,00,00, FF,00,00,00, 00,00,00,00, 00,00,00,00, 10,00,00,00, 00,C2,01,00, 00,FA,00,00
HKR,, DCB, 1, 1C,00,00,00, 00,C2,01,00, 15,20,00,00, 00,00, 0a,00, 0a,00, 08, 00, 00, 11, 13, 00, 00, 00

[PPP.AddReg] ; default / PPP
HKR, Init,      2,, "AT$IBP=HDLCP<cr>"

[X75.AddReg] ; X75
HKR, Init,      2,, "AT$IBP=X75<cr>"

[V120.AddReg] ; V120
HKR, Init,      2,, "AT$IBP=V120<cr>"

[Fallback.AddReg] ; Fallback
HKR, Init,      2,, "AT$IBP=X75FB2<cr>"

[BTX.AddReg] ; Btx
HKR, Init,      2,, "AT$IBP=BTX<cr>"

[V110.AddReg] ; V110
HKR, Init,      2,, "AT$IBP=V110<cr>"  ; 38400 baud (other rates with S271)


[EXTERNAL]
HKR,, DeviceType, 1, 01

[ISDN]
HKR, ISDN\Init, 1,,				"AT&FQ0&C1&D2<cr>"
HKR, ISDN\Init, 2,,				"ATV1\V8E0<cr>"
HKR, ISDN\NvSave,1,,				"AT&W<cr>"
HKR, Protocol\ISDN\HDLC_PPP_64K, 1,,		"AT$ibp=HDLCP$ibr=64000<cr>"
HKR, Protocol\ISDN\HDLC_PPP_56K, 1,,		"AT$ibp=HDLCP$ibr=56000<cr>"
HKR, Protocol\ISDN\X75_64K, 1,,			"AT$ibp=X75$ibr=64000<cr>"
HKR, Protocol\ISDN\X75_T_70, 1,,		"AT$ibp=X75T70<cr>"
HKR, Protocol\ISDN\V120_64K, 1,,		"AT$ibp=V120$ibr=64000<cr>"
HKR, Protocol\ISDN\V120_56K, 1,,		"AT$ibp=V120$ibr=56000<cr>"
HKR, Protocol\ISDN\AUTO_1CH, 1,,		"AT$ibp=X75FB2<cr>"
HKR, Protocol\ISDN\X75_BTX, 1,,			"AT$ibp=BTX<cr>"
HKR, Protocol\ISDN\V110_9DOT6K,1,,		"AT$ibp=V110S271.0=0S271.1=0<cr>"
HKR, Protocol\ISDN\V110_19DOT2K,1,,		"AT$ibp=V110S271.0=1S271.1=0<cr>"
HKR, Protocol\ISDN\V110_38DOT4K,1,,		"AT$ibp=V110S271.0=0S271.1=1<cr>"

HKR, ISDN\SwitchType, SWITCH_DSS1,,		"AT$IDP=DSS1<cr>"  ;DSS1 (Euro-ISDN)
HKR, ISDN\SwitchType, SWITCH_1TR6,,		"AT$IDP=1TR6<cr>"  ;1TR6 (Germany)
HKR, ISDN\SetMSN, 1  ,, 			"AT$IMSN=0,""%s"","""",""""$ICLI=0,"""",1<cr>"  ; Data port
HKR, ISDN\SetEAZ, 1 ,,   			"AT$IEAZ=0,""%s""<cr>"

; Responses

[Responses]
HKR, Responses, "0<cr>", 	1, 00, 00, 00,00,00,00, 00,00,00,00    ; OK
HKR, Responses, "1<cr>",	1, 02, 00, 00,00,00,00, 00,00,00,00    ; CONNECT
HKR, Responses, "2<cr>",	1, 08, 00, 00,00,00,00, 00,00,00,00    ; RING
HKR, Responses, "3<cr>",	1, 04, 00, 00,00,00,00, 00,00,00,00    ; NO CARRIER
HKR, Responses, "4<cr>",	1, 03, 00, 00,00,00,00, 00,00,00,00    ; ERROR
HKR, Responses, "6<cr>",	1, 05, 00, 00,00,00,00, 00,00,00,00    ; NO DIALTONE
HKR, Responses, "7<cr>",	1, 06, 00, 00,00,00,00, 00,00,00,00    ; BUSY
HKR, Responses, "8<cr>", 	1, 07, 00, 00,00,00,00, 00,00,00,00    ; NO ANSWER

HKR, Responses, "<cr><lf>CONNECT<cr><lf>",	1, 02, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>OK<cr><lf>",		1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>ERROR<cr><lf>",	1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>RING<cr><lf>",		1, 08, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO CARRIER<cr><lf>",	1, 04, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO DIALTONE<cr><lf>",	1, 05, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>BUSY<cr><lf>",		1, 06, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO ANSWER<cr><lf>",	1, 07, 00, 00,00,00,00, 00,00,00,00

; ISDN transparent no compression / no errorcorrection

HKR, Responses, "<cr><lf>CONNECT 56000<cr><lf>",	1, 02, 00, C0,DA,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 64000<cr><lf>",	1, 02, 00, 00,FA,00,00, 00,00,00,00

; ISDN V110:  no compression / no errorcorrection

HKR, Responses, "<cr><lf>CONNECT 1200/ISDN/V110<cr><lf>",	1, 02, 00, B0,04,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 2400/ISDN/V110<cr><lf>",	1, 02, 00, 60,09,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 4800/ISDN/V110<cr><lf>",	1, 02, 00, C0,12,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 9600/ISDN/V110<cr><lf>",	1, 02, 00, 80,25,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 19200/ISDN/V110<cr><lf>",	1, 02, 00, 00,4B,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 38400/ISDN/V110<cr><lf>",	1, 02, 00, 00,96,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 48000/ISDN/V110<cr><lf>",	1, 02, 00, 80,BB,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 56000/ISDN/V110<cr><lf>",	1, 02, 00, C0,DA,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 64000/ISDN/V110<cr><lf>",	1, 02, 00, 00,FA,00,00, 00,00,00,00

; ISDN HDLC/V120/X75 errorcorrection / no compression

HKR, Responses, "<cr><lf>CONNECT 56000/REL<cr><lf>",		1, 02, 02, C0,DA,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 64000/REL<cr><lf>",		1, 02, 02, 00,FA,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 56000/REL-LAPB<cr><lf>",	1, 02, 02, C0,DA,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 64000/REL-LAPB<cr><lf>",	1, 02, 02, 00,FA,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 56000/ISDN/BTX<cr><lf>",	1, 02, 02, C0,DA,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 64000/ISDN/BTX<cr><lf>",	1, 02, 02, 00,FA,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 56000/ISDN/HDLCP<cr><lf>",	1, 02, 00, C0,DA,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 64000/ISDN/HDLCP<cr><lf>",	1, 02, 00, 00,FA,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 56000/ISDN/HDLC<cr><lf>",	1, 02, 00, C0,DA,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 64000/ISDN/HDLC<cr><lf>",	1, 02, 00, 00,FA,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 56000/ISDN/V120<cr><lf>",	1, 02, 02, C0,DA,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 64000/ISDN/V120<cr><lf>",	1, 02, 02, 00,FA,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 56000/ISDN/X75<cr><lf>",	1, 02, 02, C0,DA,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 64000/ISDN/X75<cr><lf>",	1, 02, 02, 00,FA,00,00, 00,00,00,00

; ISDN independent of Transferrate: no compression / errrorcorrection

HKR, Responses, "<cr><lf>CONNECT ISDN/V110<cr><lf>",	1, 02, 02, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT ISDN/V120<cr><lf>",	1, 02, 02, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT ISDN/X75<cr><lf>",	1, 02, 02, 00,00,00,00, 00,00,00,00


