	#
	| README file for GLoria-XL
	|
	| ELSA graphics driver disk for Windows NT 4.0 build 1381. 
	|
        | Version: 5.30.05.231
        |
	| Copyright (c) 1993-97 ELSA AG, Aachen (Germany)
	|
	| ELSA AG                    Internet   : http://www.elsa.de
	| Sonnenweg 11               LocalWeb   : +49-(0)241-938800
	| D-52070 Aachen             
	|
	| ELSA Inc.                  Internet   : http://www.elsa.com
	| 2231 Calle De Luna         
	| Santa Clara, CA 95054
	| USA
	|
	| ELSA Asia Inc.             Internet   : http://www.elsa.com
	| 7F-11, No. 188, Sec. 5     
	| Nanking East Road
	| Taipei 105
	| Taiwan, R. O. C.
	|
        | ELSA Japan Inc.            Internet   : http://www.elsa.com
        | Mita Suzuki Building 3F                
        | 5-20-14 Shiba, Minato-ku
        | Tokyo 108-0014
        | Japan
        |
        | 02/27/98, CBuersch


	Table of Contents:

1       Introduction
2       List of Files
3       Installation
4       Release Notes / Known Bugs

------------------------------------------------------------------------

1       Introduction

	This file helps you with the installation of your ELSA graphics 
	adapter. It explains how to setup the ELSA WINNER driver and check
	if it has been installed properly.

1.2     Further Information
	For more information on configuring installed ELSA display drivers, 
	refer to the Windows help or the help files shipped 
	with the ELSA utilities.
	
------------------------------------------------------------------------

2       List of Files

	NOTE Not all of the files listed below can be used by your graphic
	     adapters.  Some utilities need specialized adapter capabilities
	     and hardware.

	The directory with the ELSA graphics driver for Windows NT 
	contains the following files:

	DISK1           Identifier for the first disk
	DISK2           Identifier for the second disk
	DISK3           Identifier for the third disk
	ELSA.HLP        ELSA help file
	EGLMX.INF       Script file for Microsoft setup program 
	LIESMICH.TXT    German version of the file README.TXT    
	README.TXT      This file 
	TXTSETUP.OEM    Script file for text setup while booting 
	
	Graphics display drivers:

	EGLMXM.SYS      Miniport driver
	EGLMXD.DLL      Display driver
	EMGLMXD.DLL     Multi-display driver
	EOGLL.DLL       OpenGL driver

	Utilities:

	Subdirectory Glset:
	GLSET.DLL       GLoria Settings property page
	GLSET.INF       Script file for Microsoft setup program 
	GLSET.TEX       Data file for GLoria Settings
	GLSETENG.HLP    English GLoria Settings help file 
	GLSETDEU.HLP    German GLoria Settings help file 

	Subdirectory Winmsuit:
	ELSA.HLP        ELSA help file
        ELSAENG.HLP     ELSA help file english version
        WINMPS.DLL      Applikation extension
        WINMSUIT.EXE    WINMAN Suite for faster switching of the GLoria Settings
        WINMSUIT.INF    Script file for WINMAN Suite Setup
        WSUIT_DE.DLL    Applikation extension german language

------------------------------------------------------------------------

3       Installation

3.1     Installing the ELSA Display Driver

	You can install the graphics driver using the Display Properties
	sheet.  Open the Display Property sheet and select the page 
	>>Settings<<, click on >>Display Type...<< to open the
	dialog window of the same name and select >>Change...<< in the 
	Adapter Type frame.  The >>Change Display<< dialog opens.  

	NOTE The entry >>Elsa WINNER 1000<< in this listbox will install
	     the general purpose (and less than optimal) S3 driver designed 
	     by Microsoft.  The entries in the Manufacturer's >>S3<< list can 
	     be used but do not always work properly.  General purpose 
	     drivers are installed here as well!

	Click the button >>Have Disk...<< to install the ELSA drivers. 
	Windows NT prompts you to enter the disk with the driver or browse
	for the path.  Select >>Browse...<< when installing from CD-ROM and 
	locate the file ELSA.INF for the driver suitable for your hardware.  
	When installing from floppy disk, insert the first driver disk.
	Select the >>OK<< button.

	A list box appears. Here, choose the entry matching your graphics
	adapter and click >>OK<<.  Confirm the >>Third-party Drivers<<
	dialog with >>Yes<<.

	The driver files and utilities are now copied and installed to 
	your hard disk.  When installing from floppies, the >>Insert Disk<< 
	dialog prompts you when the disk has to be changed.

	The >>Installing Driver<< window informs you that the driver has 
	been installed. Confirm this message and close all display 
	settings windows until you are asked to reboot your computer.

	NOTE With Windows NT 4.0, graphic drivers cannot be loaded
	     dynamically. This is not an ELSA limitation. 

	To activate the ELSA driver the computer has to be restarted. 
	Please press >>Yes<< in the >>System Settings Change<< dialog.
	When you've selected to restart, the system will reboot and 
	the initial installation is finished.

	NOTE Windows NT 4.0 will now restart in a resolution of 
	     640*480 pixel at 256 colors and 60Hz refresh, unless you have
	     updated your driver in which case the previous resolution is 
	     taken over.  Refer to your Windows NT Help on how to change the 
	     display properties settings.

	After Windows NT is restarted, the dialog >>Registry Editor<< 
	informs you that some information has been entered into the
	registry. This was done to install the display property pages.

	Simultaneously the Display Properties sheet opens with the 
	>>Settings<< page and a dialog >>Invalid Display Settings<<
	which tells you that a new driver was installed and that you have
	to select your preferred display resolution. 
	
3.2     Installation of the ELSA GLoria Settings

	The ELSA GLoria Settings can be easily installed from the Explorer by clicking 
        the right mouse button on the appropriate GLSET.INF file in the directory "ALPHA\GLSET" 
        in the source-path for the driver-installation and then selecting "Install...". 
	
	NOTE: For deinstallation of the GLoria Settings, choose  "Add/Remove Programs" 
     	      in Control Panel.

3.3     Installation of the ELSA Winman Suite

	The ELSA Winman Suite can be easily installed from the Explorer by clicking 
        the right mouse button on the appropriate WINMSUIT.INF file in the directory "ALPHA\WINMSUIT" 
        in the source-path for the driver-installation and then selecting "Install...". 
	After the installation the system has to be rebooted for the utility to appear in the 
        task bar. Alternatively, you can start the file WINMSUIT.EXE in your
        "WINDOWS NT\ELSAUTIL" directory.
	
	NOTE: For deinstallation of the Winman Suite, choose  "Add/Remove Programs" 
     	      in Control Panel.

-----------------------------------------------------------------------------------------------

4       Release Notes / Known Bugs

4.1	Release Notes

        First release

4.2     Known bugs
                        PRO/E Graphics Short Check:
			Hidden lines may be visible
			With 3D extensions deactivated it may happen that sketches are not visible.
			Sketches may become black cubes while rotating/zooming/panning.
			
