        #
        | README file for
        |
        | ELSA Windows NT4.0 Driver Disk, ver 4.00.00.0104
        |
        |       VICTORY II
        |
        | (c) 1999 ELSA AG, (Aachen, Germany)
        |
        | ELSA AG                  Internet   : http://www.elsa.de
        | Sonnenweg 11             LocalWeb   : +49-(0)241-938800
        | D-52070 Aachen           
        |
        | ELSA Inc.                Internet   : http://www.elsa.com
        | 2231 Calle De Luna       
        | Santa Clara, CA 95054
        | USA
        |
        | ELSA Asia Inc.           Internet   : http://www.elsa.com
        | 7F-11, No. 188, Sec. 5   
        | Nanking East Road
        | Taipei 105
        | Taiwan, R. O. C.
        |
        | ELSA Japan Inc.          Internet   : http://www.elsa.com
        | Mita Suzuki Building 3F  
        | 5-20-14 Shiba, Minato-ku
        | Tokyo 108-0014
        | Japan
        |
        | 01/25/99, MKreiten


        Contents

        1. Overview
        2. Contents
        3. Installation
        4. History
        5. Release Notes
        6. Known Bugs and Operating Notes


------------------------------------------------------------------------

1.      Overview

        This CD contains the ELSA Display Driver for Microsoft
        Windows NT4.0

        The driver supports 256, 65536 and 16 Million colors
        in all resolutions available on used ELSA board.


------------------------------------------------------------------------

2.      Contents

        This directory contains the following files:

        README.TXT      the file you currently look at
        LIESMICH.TXT    german version of README

        VERSION.TXT     version info about driver and tools
        ELSAVII.INF     Installation file for driver and tools
        ELSAVIID.DLL    NT Display Treiber
        ELSAVIIM.SYS    NT Display Treiber (Miniport)
	GLIDE2X.DLL	3Dfx Glide 2.6
	GLIDE3X.DLL	3Dfx Glide 3.1
	3DFXSPL3.DLL	3Dfx Glide Splash screen
        WINMAN.DLL      Control Panel ELSA Settings
        WINMAN.EXE      Control Panel ELSA Settings
        WINMAN.MON      Control Panel ELSA Settings
        WINMANDE.CNT    Contents German Help for Control Panel ELSA Settings
        WINMANDE.HLP    German Help for Control Panel ELSA Settings
        WINMANEN.CNT    Contents English Help for Control Panel ELSA Settings
        WINMANEN.HLP    English Help for Control Panel ELSA Settings
        WINMANES.HLP    Spanish Help for Control Panel ELSA Settings
        WINMANFR.CNT    Contents French Help for Control Panel ELSA Settings
        WINMANFR.HLP    French Help for Control Panel ELSA Settings
        WINMANIT.HLP    Italien Help for Control Panel ELSA Settings
        WINMANJA.CNT    Contents Japanese Help for Control Panel ELSA Settings
        WINMANJA.HLP    Japanese Help for Control Panel ELSA Settings
        WINMANNL.HLP    Dutch Help for Control Panel ELSA Settings
        WINMANSV.HLP    Swedish Help for Control Panel ELSA Settings

        In case of trouble during or after installation, please make
        sure you have all the files mentioned above!


------------------------------------------------------------------------


3.      Installation


3.1     Manual installation of ELSA Display Driver
        

        - Start the dialog "Properties for Display" by clicking right
          mouse button on the desktop or select per Control Panel 
          -> "Display".

        - Select the Property Page "Settings" 

        - Click on "Display Type"

        - Push the button "Change...". A dialog "Change Display" will 
          pop up.

        - Push the button "Have Disk..." and "Browse..."

        - change to the Victory2 - directory on the WINNERware CD.

        - Select your ELSA display adapter in the "Devices" list.

        - Close the dialog "Chang Display". At this time the
          screen may flicker for a moment. This is not a bug! Windows 
          is trying to find out, which graphics modes are available with
          this driver.

        - Please answer the following questions with "OK", "Close" or 
          "Apply" and reboot the system.

        - Now you can select resolution and color depth in the main
          dialog "Properties for Display". For the first installation
          you should select 1024x768 in HiColor. This configuration
          is available for all memory configurations on all ELSA
          Boards.

        - Close "Properties for Display" by "OK" or "Apply

        After the restart the configuration of the ELSA display adapter
        driver starts from the Windows desktop.
 
        
        - Start the dialog "Properties for Display" by clicking right
          mouse button on the desktop or per Control Panel -> Display.
        - Select the Property Page "Settings" or "ELSA Settings".
        - Property Page Settings:
          Standard-Windows-Dialog for changing resolution, color
          depth and font size.
        - Property Page ELSA Settings:
          ELSA Settings gives you full control to configure your ELSA
          display adapter perfectly. You can change resolution, color
          depth and refresh rate.


------------------------------------------------------------------------

4.      Revision History

        This section describes changes to the previous releases of
        this disk.

        Version 4.00.00.0104
        - first released ELSA driver


------------------------------------------------------------------------

5.      Release notes

        

------------------------------------------------------------------------

6.      Known Bugs and Operating Notes

        This section documents known anomalies or problems and gives
        hints on work arounds.

        The display driver requires at least service pack 3 installed !
        Service pack 4 can be found on the WINNERware CD

        This display driver is for singlescreen use only.

------------------------------------------------------------------------
