
[Version]
Signature = $Windows NT$
Class     = Net
ClassGUID = {4D36E972-E325-11CE-BFC1-08002BE10318}
Provider  = %V_ELSA%
DriverVer = %V_DATE%,%V_VERSION%

[Manufacturer]
%V_ELSA% = ELSA

[ClassInstall]

[ControlFlags]

[ELSA]
%ELSAWAN.DeviceDesc% = ELSAWAN.ndi, ELSAWAN

[ELSAWAN.ndi]
DriverVer       = %V_DATE%,%V_VERSION%
AddReg          = ELSAWAN.ndis.reg, ELSAWAN.95.reg
CopyFiles       = ELSAWAN.CopyFiles

[ELSAWAN.ndi.NT]
DriverVer       = %V_DATE%,%V_VERSION%
AddReg          = ELSAWAN.ndis.reg, ELSAWAN.nt.reg
Characteristics = 0x9  ; NCF_VIRTUAL NCF_HIDDEN
CopyFiles       = ELSAWAN.CopyFiles.NT

[ELSAWAN.ndis.reg]
HKR, ,                    BoardType,        0,       "ELSAWAN"
HKR, ,                    BoardName,        0,       "ELSAWAN"
HKR, Ndi,                 HelpText,         0,       %V_DESC%
HKR, Ndi\Interfaces,      DefUpper,         0,       "ndiswan"
HKR, Ndi\Interfaces,      DefLower,         0,       "isdn"
HKR, Ndi\Interfaces,      UpperRange,       0,       "ndiswan"
HKR, Ndi\Interfaces,      LowerRange,       0,       "isdn"

[ELSAWAN.95.reg]
HKR, ,                    DevLoader,        0,       "*ndis"
HKR, ,                    DeviceVxDs,       0,       "ELSAWAN.sys"
HKR, ,                    EnumPropPages,    0,       "netdi.dll,EnumPropPages"
HKR, ,                    DeviceName,       0,       "ELSAWAN"
HKR, ,                    NumberOfLines,    0,       "1"
HKR, Ndi,                 DeviceID,         0,       "ELSAWAN"
HKR, Ndi\Compatibility,   RequireAll,       0,       "NDISWAN"

HKR, NDIS,                LogDriverName,    0,       "ELSAWAN"
HKR, NDIS,                MajorNdisVersion, 0x10001, 05
HKR, NDIS,                MinorNdisVersion, 0x10001, 00

HKR, TAPI,                Properties,       1,       00,00,00,00
HKR, TAPI,                DeviceCaps,       1,       14,00,00,00, 00,00,00,00, 00,00,00,00, 01,00,00,00, 00,00,00,00
HKR, TAPI\Line0,          Properties,       1,       00,00,00,00
HKR, TAPI\Line0,          SwitchType,       1,       00,00,00,00
HKR, TAPI\Line0,          LineCaps,         1,       1c,00,00,00, 00,00,00,00, 03,00,00,00, 01,00,00,00, 03,00,00,00, 02,00,00,00, 00,00,00,00
HKR, TAPI\Line0\Channel0, Properties,       1,       00,00,00,00
HKR, TAPI\Line0\Channel0, ChannelCaps,      1,       00,00,00,00
HKR, TAPI\Line0\Channel0, SPID,             0,       ""
HKR, TAPI\Line0\Channel0, Phone,            0,       ""
HKR, TAPI\Line0\Channel1, Properties,       1,       00,00,00,00
HKR, TAPI\Line0\Channel1, ChannelCaps,      1,       00,00,00,00
HKR, TAPI\Line0\Channel1, SPID,             0,       ""
HKR, TAPI\Line0\Channel1, Phone,            0,       ""

[ELSAWAN.nt.reg]
HKR, ,                    WanEndPoints,     0x10001, 2
HKR, ,                    IsdnNumDChannels, 0x10001, 1
HKR, ,                    IsdnSwitchTypes,  0x10000, "Auto"
HKR, 0,                   IsdnNumBChannels, 0x10001, 2
HKR, 0,                   IsdnSwitchType,   0x10001, 0
HKR, Ndi,                 Service,          0,       "ELSAWAN"

[DestinationDirs]
ELSAWAN.CopyFiles    = 11
ELSAWAN.CopyFiles.NT = 12

[ELSAWAN.CopyFiles]
ELSAWAN.sys,,,4

[ELSAWAN.CopyFiles.NT]
ELSAWAN.sys,,,4

[ELSAWAN.ndi.NT.Services]
AddService = ELSAWAN, 2, ELSAWAN.Service

[ELSAWAN.Service]
DisplayName     = %ELSAWAN.DeviceDesc% (Ver. %V_VERSION%)
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 2 ;%SERVICE_AUTO_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\ELSAWAN.sys
LoadOrderGroup  = NDIS

[SourceDisksNames]
1 = "ELSA LANCOM Software CD", "",

[SourceDisksFiles]
ELSAWAN.sys = 1

[Strings]
V_ELSA              = "ELSA"
ELSAWAN.DeviceDesc  = "ELSA COMCAPI (NDISWAN MiniPort)"
V_DATE              = "01/14/2000"
V_VERSION           = "3.02.0005"
V_DESC              = "ELSA NDISWAN MiniPort Driver for CAPI 2.0"
